IFC building model
Schema: "IFC4X3_ADD2"
Description: "ViewDefinition [ReferenceView]"
File name: "Building-Architecture.ifc"
Time stamp: "2024-11-14T11:09:35"
Preprocessor: "IFC-manager for SketchUp (5.3.3)"
Originating system: "SketchUp 2024 (24.0.594)"
Authorization: "None"
Application: "IFC manager for sketchup" version "5.3.3" identifier "su_ifcmanager" by Organization "BIM-Tools"

People and organizations
  Person "Jan B." id "3720f2e9-0107-4ce6-b699-e20d9bd03331" of Organization "buildingSMART International" description "buildingSMART is the worldwide industry body driving the digital transformation of the built environment."
  Owner history of Person "Jan B." id "3720f2e9-0107-4ce6-b699-e20d9bd03331" of Organization "buildingSMART International" description "buildingSMART is the worldwide industry body driving the digital transformation of the built environment." | application "IFC manager for sketchup" version "5.3.3" identifier "su_ifcmanager" by Organization "BIM-Tools" | change ADDED | created 1731578975 (2024-11-14T10:09:35Z) | last modified 1731578975 (2024-11-14T10:09:35Z) by Person "Jan B." id "3720f2e9-0107-4ce6-b699-e20d9bd03331" of Organization "buildingSMART International" description "buildingSMART is the worldwide industry body driving the digital transformation of the built environment." with "IFC manager for sketchup" version "5.3.3" identifier "su_ifcmanager" by Organization "BIM-Tools"

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE

Spatial structure
IFCPROJECT "ifc silly sample scene - project" | description "Demystifying IFC with a playful scene using diverse building elements and compositions."
  IFCSITE "environment - site" | COMPLEX | elevation above sea level 0. | description "A sample scene environment, showcasing the surrounding landscape."
    contains 1 element
      1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "geo-reference" | object type "origin" | names: "geo-reference" | descriptions: "The reference point for transforming the local engineering coordinate system into the coordinate reference system of the underlying map." | material: "virtual_black"
    IFCSITE "house - site" | PARTIAL | elevation above sea level 0. | description "Smoke curls from a friendly chimney, promising warmth within this idyllic hilltop house."
      contains 1 element
        1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "origin" | object type "origin" | names: "origin" | descriptions: "The local position for coordination of aspect models." | material: "virtual_white"
      IFCBUILDING "Single-family house" | reference height above sea level 0. | terrain above sea level 0. | description "The main building structure, providing shelter and space."
        contains 3 elements
          1 x IFCROOF | type IFCROOFTYPE "house - roof" | object type "gable_roof" | names: "house - roof" | descriptions: "A sturdy roof, sheltering the house from the elements." | parts: 2 IFCSLAB
          1 x IFCSPATIALZONE | type IFCSPATIALZONETYPE "house - gross volume" | object type "gross volume" | names: "house - gross volume"
          1 x IFCEARTHWORKSFILL | object type "subgrade" | SUBGRADE | names: "sand bedding" | descriptions: "A layer of ground floor sand bedding, providing a stable base." | material: "bulk-material_sand-coarse_generic"
        IFCBUILDINGSTOREY "00 groundfloor" | description "The ground floor, forming the base level of the building."
          contains 7 elements
            1 x IFCSLAB | type IFCSLABTYPE "house - groundfloor" | object type "slab on grade" | names: "floor" | descriptions: "A solid, site-cast concrete floor, providing a strong foundation." | material: "concrete_reinforced_in-situ" | property sets: Pset_SlabCommon, Qto_SlabBaseQuantities
            1 x IFCWALL | type IFCWALLTYPE "house - outer wall - house right front" | object type "solidwall" | names: "house - outer wall - house right front" | descriptions: "A solid outer wall, forming the right front side of the house." | material: "stone_sand-lime" | property sets: Qto_WallBaseQuantities
            1 x IFCWALL | type IFCWALLTYPE "house - outer wall - house right back" | object type "solidwall" | names: "house - outer wall - house right back" | descriptions: "A solid outer wall, forming the right back side of the house." | material: "stone_sand-lime" | property sets: Qto_WallBaseQuantities
            1 x IFCWALL | type IFCWALLTYPE "house - outer wall - house left" | object type "solidwall" | names: "house - outer wall - house left" | descriptions: "A solid outer wall, forming the left side of the house." | material: "stone_sand-lime" | property sets: Qto_WallBaseQuantities
            1 x IFCCHIMNEY | type IFCCHIMNEYTYPE "house - chimney" | object type "flue" | names: "house - chimney" | descriptions: "A chimney, standing tall and proud, guiding smoke away from the home." | material: "stone_sand-lime"
            1 x IFCBUILDINGELEMENTPROXY | names: "Group#19" | material: "Default"
            1 x IFCWALL | type IFCWALLTYPE "plumbing wall" | object type "plumbingwall" | names: "plumbing wall" | descriptions: "A wall designed to house and protect plumbing systems, keeping the pipes snug and secure." | material: "gypsum_fiber-board_panel" | property sets: Qto_WallBaseQuantities
          IFCSPACE "living room" | object type "living area" | description "A cozy space, perfect for relaxation and family gatherings."
            contains 2 elements
              1 x IFCFURNITURE | type IFCFURNITURETYPE "house - kitchen" | object type "kitchen" | names: "kitchen" | descriptions: "The heart of the home, where meals are prepared and shared." | material: "wood_mdf_plate"
              1 x IFCBUILDINGELEMENTPROXY | names: "Group#18" | material: "Default"
          IFCSPACE "entry hall" | object type "hallway" | description "A welcoming entry hall, the first impression of the home."

Types
  IFCBUILDINGELEMENTPROXYTYPE "geo-reference" | element type "origin" | USERDEFINED | 1 occurrence | description "The reference point for transforming the local engineering coordinate system into the coordinate reference system of the underlying map."
  IFCBUILDINGELEMENTPROXYTYPE "origin" | element type "origin" | USERDEFINED | 1 occurrence | description "The local position for coordination of aspect models."
  IFCROOFTYPE "house - roof" | element type "gable_roof" | GABLE_ROOF | 1 occurrence | description "A sturdy roof, sheltering the house from the elements."
  IFCSPATIALZONETYPE "house - gross volume" | element type "gross volume" | USERDEFINED | 1 occurrence
  IFCSLABTYPE "house - groundfloor" | element type "slab on grade" | FLOOR | 1 occurrence | property sets: Pset_SlabCommon | description "A solid, site-cast concrete floor, providing a strong foundation."
  IFCWALLTYPE "house - outer wall - house right front" | element type "solidwall" | SOLIDWALL | 1 occurrence | description "A solid outer wall, forming the right front side of the house."
  IFCWALLTYPE "house - outer wall - house right back" | element type "solidwall" | SOLIDWALL | 1 occurrence | description "A solid outer wall, forming the right back side of the house."
  IFCWALLTYPE "house - outer wall - house left" | element type "solidwall" | SOLIDWALL | 1 occurrence | description "A solid outer wall, forming the left side of the house."
  IFCCHIMNEYTYPE "house - chimney" | element type "flue" | USERDEFINED | 1 occurrence | description "A chimney, standing tall and proud, guiding smoke away from the home."
  IFCWALLTYPE "plumbing wall" | element type "plumbingwall" | PLUMBINGWALL | 1 occurrence | description "A wall designed to house and protect plumbing systems, keeping the pipes snug and secure."
  IFCFURNITURETYPE "house - kitchen" | element type "kitchen" | USERDEFINED | 1 occurrence | description "The heart of the home, where meals are prepared and shared."

Property sets
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    AcousticRating = "29dB Rw" (IFCLABEL)
    FireRating = "REI30" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
  Pset_SlabCommon | properties | on 1 type object
    FireRating = "REI60" (IFCLABEL)
    SurfaceSpreadOfFlame = "A2 s1 d0" (IFCLABEL)
  Qto_SlabBaseQuantities | quantities | on 1 object (1 IFCSLAB)
    Depth = 250.00000000009484 [MILLI METRE]
    NetArea = 25.749999999991743 [SQUARE_METRE]
    NetVolume = 6.437500000000378 [CUBIC_METRE]
  Qto_SlabBaseQuantities | quantities | on 1 object (1 IFCSLAB)
    Depth = 300.0000000001534 [MILLI METRE]
    NetArea = 22.40114282797721 [SQUARE_METRE]
    NetVolume = 6.7203428483966 [CUBIC_METRE]
  Qto_SlabBaseQuantities | quantities | on 1 object (1 IFCSLAB)
    Depth = 300.0000000000386 [MILLI METRE]
    NetArea = 31.211693321568944 [SQUARE_METRE]
    NetVolume = 9.36350799647189 [CUBIC_METRE]
  Qto_WallBaseQuantities | quantities | on 1 object (1 IFCWALL)
    Length = 1799.9999999999711 [MILLI METRE]
    NetSideArea = 6.346324676317877 [SQUARE_METRE]
    NetVolume = 1.26926493526358 [CUBIC_METRE]
    Width = 200.0000000000007 [MILLI METRE]
  Qto_WallBaseQuantities | quantities | on 1 object (1 IFCWALL)
    Length = 4200.000000000067 [MILLI METRE]
    NetSideArea = 8.928090911402801 [SQUARE_METRE]
    NetVolume = 1.7856181822821586 [CUBIC_METRE]
    Width = 200.00000000017903 [MILLI METRE]
  Qto_WallBaseQuantities | quantities | on 1 object (1 IFCWALL)
    Length = 6000.000000000036 [MILLI METRE]
    NetSideArea = 21.154415587728412 [SQUARE_METRE]
    NetVolume = 4.230883117545889 [CUBIC_METRE]
    Width = 200.00000000000975 [MILLI METRE]
  Qto_WallBaseQuantities | quantities | on 1 object (1 IFCWALL)
    Length = 3800.000000000086 [MILLI METRE]
    NetSideArea = 6.862581386977263 [SQUARE_METRE]
    NetVolume = 0.16470195328802126 [CUBIC_METRE]
    Width = 24.000000000082615 [MILLI METRE]