IFC building model
Schema: "IFC4X3_ADD2"
Description: "ViewDefinition [ReferenceView]"
File name: "Building-Structural.ifc"
Time stamp: "2024-11-14T11:09:35"
Preprocessor: "IFC-manager for SketchUp (5.3.3)"
Originating system: "SketchUp 2024 (24.0.594)"
Authorization: "None"
Application: "IFC manager for sketchup" version "5.3.3" identifier "su_ifcmanager" by Organization "BIM-Tools"

People and organizations
  Person "Jan B." id "3720f2e9-0107-4ce6-b699-e20d9bd03331" of Organization "buildingSMART International" description "buildingSMART is the worldwide industry body driving the digital transformation of the built environment."
  Owner history of Person "Jan B." id "3720f2e9-0107-4ce6-b699-e20d9bd03331" of Organization "buildingSMART International" description "buildingSMART is the worldwide industry body driving the digital transformation of the built environment." | application "IFC manager for sketchup" version "5.3.3" identifier "su_ifcmanager" by Organization "BIM-Tools" | change ADDED | created 1731578975 (2024-11-14T10:09:35Z) | last modified 1731578975 (2024-11-14T10:09:35Z) by Person "Jan B." id "3720f2e9-0107-4ce6-b699-e20d9bd03331" of Organization "buildingSMART International" description "buildingSMART is the worldwide industry body driving the digital transformation of the built environment." with "IFC manager for sketchup" version "5.3.3" identifier "su_ifcmanager" by Organization "BIM-Tools"

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE

Spatial structure
IFCPROJECT "ifc silly sample scene - project" | description "Demystifying IFC with a playful scene using diverse building elements and compositions."
  IFCSITE "environment - site" | COMPLEX | elevation above sea level 0. | description "A sample scene environment, showcasing the surrounding landscape."
    contains 1 element
      1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "geo-reference" | object type "origin" | names: "geo-reference" | descriptions: "The reference point for transforming the local engineering coordinate system into the coordinate reference system of the underlying map." | material: "virtual_black"
    IFCSITE "house - site" | PARTIAL | elevation above sea level 0. | description "Smoke curls from a friendly chimney, promising warmth within this idyllic hilltop house."
      contains 1 element
        1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "origin" | object type "origin" | names: "origin" | descriptions: "The local position for coordination of aspect models." | material: "virtual_white"
      IFCBUILDING "Single-family house" | reference height above sea level 0. | terrain above sea level 0. | description "The main building structure, providing shelter and space."
        contains 1 element
          1 x IFCROOF | type IFCROOFTYPE "house - roof" | object type "gable_roof" | names: "house - roof" | descriptions: "A sturdy roof, sheltering the house from the elements." | parts: 6 IFCBEAM, 2 IFCDISCRETEACCESSORY
        IFCBUILDINGSTOREY "00 groundfloor" | description "The ground floor, forming the base level of the building."
          contains 7 elements
            1 x IFCFOOTING | type IFCFOOTINGTYPE "house - foundation" | object type "strip_footing" | names: "house - foundation" | descriptions: "A house strip footing, ensuring stability and support." | material: "concrete_reinforced_in-situ"
            1 x IFCWALL | type IFCWALLTYPE "house - outer wall - house back" | object type "solidwall" | names: "house - outer wall - house back" | descriptions: "A solid outer wall, forming the back of the house." | material: "stone_sand-lime" | property sets: Qto_WallBaseQuantities
            1 x IFCWALL | type IFCWALLTYPE "house - outer wall - house front" | object type "solidwall" | names: "house - outer wall - house front" | descriptions: "A solid outer wall, forming the front of the house." | material: "stone_sand-lime" | property sets: Qto_WallBaseQuantities
            1 x IFCWALL | type IFCWALLTYPE "house - outer wall - house front right" | object type "solidwall" | names: "house - outer wall - house front right" | descriptions: "A solid outer wall, forming the front right side of the house." | material: "stone_sand-lime" | property sets: Qto_WallBaseQuantities
            1 x IFCCHIMNEY | type IFCCHIMNEYTYPE "house - chimney" | object type "flue" | names: "house - chimney" | descriptions: "A chimney, standing tall and proud, guiding smoke away from the home." | material: "stone_sand-lime"
            1 x IFCBUILDINGELEMENTPROXY | names: "Group#21" | material: "Default"
            1 x IFCWALL | type IFCWALLTYPE "house - inner wall" | object type "solidwall" | names: "house - inner wall" | descriptions: "A solid inner wall, providing structural support within the house." | material: "stone_sand-lime" | property sets: Qto_WallBaseQuantities

Types
  IFCBUILDINGELEMENTPROXYTYPE "geo-reference" | element type "origin" | USERDEFINED | 1 occurrence | description "The reference point for transforming the local engineering coordinate system into the coordinate reference system of the underlying map."
  IFCBUILDINGELEMENTPROXYTYPE "origin" | element type "origin" | USERDEFINED | 1 occurrence | description "The local position for coordination of aspect models."
  IFCROOFTYPE "house - roof" | element type "gable_roof" | GABLE_ROOF | 1 occurrence | description "A sturdy roof, sheltering the house from the elements."
  IFCFOOTINGTYPE "house - foundation" | element type "strip_footing" | STRIP_FOOTING | 1 occurrence | description "A house strip footing, ensuring stability and support."
  IFCWALLTYPE "house - outer wall - house back" | element type "solidwall" | SOLIDWALL | 1 occurrence | description "A solid outer wall, forming the back of the house."
  IFCWALLTYPE "house - outer wall - house front" | element type "solidwall" | SOLIDWALL | 1 occurrence | description "A solid outer wall, forming the front of the house."
  IFCWALLTYPE "house - outer wall - house front right" | element type "solidwall" | SOLIDWALL | 1 occurrence | description "A solid outer wall, forming the front right side of the house."
  IFCCHIMNEYTYPE "house - chimney" | element type "flue" | USERDEFINED | 1 occurrence | description "A chimney, standing tall and proud, guiding smoke away from the home."
  IFCWALLTYPE "house - inner wall" | element type "solidwall" | SOLIDWALL | 1 occurrence | description "A solid inner wall, providing structural support within the house."

Property sets
  Qto_WallBaseQuantities | quantities | on 1 object (1 IFCWALL)
    Length = 5200.000000000204 [MILLI METRE]
    NetSideArea = 21.43257684268954 [SQUARE_METRE]
    NetVolume = 4.28651536853961 [CUBIC_METRE]
    Width = 200.0000000000794 [MILLI METRE]
  Qto_WallBaseQuantities | quantities | on 1 object (1 IFCWALL)
    Length = 3800.0000000000714 [MILLI METRE]
    NetSideArea = 14.65654653888909 [SQUARE_METRE]
    NetVolume = 2.9313093077792742 [CUBIC_METRE]
    Width = 200.00000000009933 [MILLI METRE]
  Qto_WallBaseQuantities | quantities | on 1 object (1 IFCWALL)
    Length = 1299.9999999999152 [MILLI METRE]
    NetSideArea = 3.7284567106731448 [SQUARE_METRE]
    NetVolume = 0.7456913421348146 [CUBIC_METRE]
    Width = 200.0000000000498 [MILLI METRE]
  Qto_WallBaseQuantities | quantities | on 1 object (1 IFCWALL)
    Length = 3900.000000000167 [MILLI METRE]
    NetSideArea = 15.222870132019404 [SQUARE_METRE]
    NetVolume = 3.044574026405024 [CUBIC_METRE]
    Width = 200.00000000007506 [MILLI METRE]
  Qto_BeamBaseQuantities | quantities | on 1 object (1 IFCBEAM)
    CrossSectionArea = 0.020000000000000465 [SQUARE_METRE]
    Length = 2699.9999999999427 [MILLI METRE]
    NetVolume = 0.05400000000000011 [CUBIC_METRE]
  Qto_BeamBaseQuantities | quantities | on 1 object (1 IFCBEAM)
    CrossSectionArea = 0.02000000000000047 [SQUARE_METRE]
    Length = 5799.999999999974 [MILLI METRE]
    NetVolume = 0.1160000000000022 [CUBIC_METRE]
  Qto_BeamBaseQuantities | quantities | on 1 object (1 IFCBEAM)
    CrossSectionArea = 0.020000000000000465 [SQUARE_METRE]
    Length = 599.9999999999343 [MILLI METRE]
    NetVolume = 0.011999999999998965 [CUBIC_METRE]
  Qto_BeamBaseQuantities | quantities | on 1 object (1 IFCBEAM)
    CrossSectionArea = 0.02000000000000046 [SQUARE_METRE]
    Length = 3999.9999999999313 [MILLI METRE]
    NetVolume = 0.08000000000000046 [CUBIC_METRE]
  Qto_BeamBaseQuantities | quantities | on 1 object (1 IFCBEAM)
    CrossSectionArea = 0.020000000000000465 [SQUARE_METRE]
    Length = 5799.999999999974 [MILLI METRE]
    NetVolume = 0.11600000000000217 [CUBIC_METRE]
  Qto_BeamBaseQuantities | quantities | on 1 object (1 IFCBEAM)
    CrossSectionArea = 0.020000000000000472 [SQUARE_METRE]
    Length = 5799.999999999974 [MILLI METRE]
    NetVolume = 0.11600000000000223 [CUBIC_METRE]