IFC building model
Schema: "IFC4X3_ADD2"
Description: "ViewDefinition [ReferenceView]"
File name: "Infra-Bridge.ifc"
Time stamp: "2025-02-27T11:09:37"
Preprocessor: "IFC-manager for SketchUp (5.3.3)"
Originating system: "SketchUp 2024 (24.0.594)"
Authorization: "None"
Application: "IFC manager for sketchup" version "5.3.3" identifier "su_ifcmanager" by Organization "BIM-Tools"

People and organizations
  Person "Jan B." id "3720f2e9-0107-4ce6-b699-e20d9bd03331" of Organization "buildingSMART International" description "buildingSMART is the worldwide industry body driving the digital transformation of the built environment."
  Owner history of Person "Jan B." id "3720f2e9-0107-4ce6-b699-e20d9bd03331" of Organization "buildingSMART International" description "buildingSMART is the worldwide industry body driving the digital transformation of the built environment." | application "IFC manager for sketchup" version "5.3.3" identifier "su_ifcmanager" by Organization "BIM-Tools" | change ADDED | created 1731578976 (2024-11-14T10:09:36Z) | last modified 1731578976 (2024-11-14T10:09:36Z) by Person "Jan B." id "3720f2e9-0107-4ce6-b699-e20d9bd03331" of Organization "buildingSMART International" description "buildingSMART is the worldwide industry body driving the digital transformation of the built environment." with "IFC manager for sketchup" version "5.3.3" identifier "su_ifcmanager" by Organization "BIM-Tools"

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE

Spatial structure
IFCPROJECT "ifc silly sample scene - project" | description "Demystifying IFC with a playful scene using diverse building elements and compositions."
  IFCSITE "environment - site" | COMPLEX | elevation above sea level 0. | description "A sample scene environment, showcasing the surrounding landscape."
    contains 1 element
      1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "geo-reference" | object type "origin" | names: "geo-reference" | descriptions: "The reference point for transforming the local engineering coordinate system into the coordinate reference system of the underlying map." | material: "virtual_black"
    IFCSITE "road parking - site" | PARTIAL | elevation above sea level 0. | description "A designated parking area, providing space for vehicles."
    IFCSITE "road river bridge - site" | PARTIAL | elevation above sea level 0. | description "The site of the road river bridge, connecting different areas."
      IFCBRIDGE "road river bridge" | object type "girder" | GIRDER | description "A sturdy bridge, spanning the river and connecting roads."
        IFCBRIDGEPART "road rail bridge - approach" | object type "approach" | COMPLEX | LATERAL | description "The approach to the road rail bridge, ensuring a smooth transition."
          contains 1 element
            1 x IFCSLAB | type IFCSLABTYPE "bridge road - approach slab" | names: "bridge road - approach slab" | descriptions: "A solid slab, ensuring a smooth transition, the bridge's welcome mat." | material: "concrete_reinforced_prefab" | property sets: Qto_SlabBaseQuantities
          IFCBRIDGEPART "bridge road - abutment" | object type "abutment" | PARTIAL | LATERAL | ABUTMENT | description "A strong abutment, providing essential support for the bridge road."
            contains 1 element
              1 x IFCBEAM | type IFCBEAMTYPE "road river bridge - abutment support beam" | object type "beam" | names: "road river bridge - abutment support beam" | descriptions: "A strong support beam, providing stability to the bridge abutment." | material: "concrete_reinforced_in-situ" | property sets: Qto_BeamBaseQuantities
        IFCBRIDGEPART "road rail bridge - approach" | object type "approach" | COMPLEX | LATERAL | description "The approach to the road rail bridge, ensuring a smooth transition."
          contains 1 element
            1 x IFCSLAB | type IFCSLABTYPE "bridge road - approach slab" | names: "bridge road - approach slab" | descriptions: "A solid slab, ensuring a smooth transition, the bridge's welcome mat." | material: "concrete_reinforced_prefab" | property sets: Qto_SlabBaseQuantities
          IFCBRIDGEPART "bridge road - abutment" | object type "abutment" | PARTIAL | LATERAL | ABUTMENT | description "A strong abutment, providing essential support for the bridge road."
            contains 1 element
              1 x IFCBEAM | type IFCBEAMTYPE "road river bridge - abutment support beam" | object type "beam" | names: "road river bridge - abutment support beam" | descriptions: "A strong support beam, providing stability to the bridge abutment." | material: "concrete_reinforced_in-situ" | property sets: Qto_BeamBaseQuantities
        IFCBRIDGEPART "road rail bridge - deck" | object type "deck" | LATERAL | DECK | description "The deck, providing a stable surface for vehicles and trains on the road rail bridge."
          contains 3 elements
            2 x IFCRAILING | type IFCRAILINGTYPE "bridge road railing" | object type "guardrail" | names: "bridge road railing" | descriptions: "A protective railing, ensuring safety along the bridge road." | material: "wood-generic"
            1 x IFCSLAB | type IFCSLABTYPE "road river bridge - bridge deck" | object type "floor" | names: "road river bridge - bridge deck" | descriptions: "The bridge deck, providing a stable surface for vehicles to cross the river." | material: "wood-generic" | property sets: Qto_SlabBaseQuantities
        IFCBRIDGEPART "road rail bridge - superstructure" | object type "superstructure" | LATERAL | SUPERSTRUCTURE | description "The superstructure, forming the main body of the road rail bridge."
          contains 3 elements
            3 x IFCBEAM | type IFCBEAMTYPE "road river bridge - main girder" | object type "girder_segment" | names: "road river bridge - main girder" | descriptions: "The main girder, providing essential support for the road river bridge." | material: "wood-generic"
        IFCBRIDGEPART "road river bridge - substructure" | object type "substructure" | COMPLEX | LATERAL | SUBSTRUCTURE | description "The substructure, providing essential support for the road river bridge."
          IFCBRIDGEPART "road river bridge - pier" | object type "pier" | PARTIAL | LATERAL | PIER | description "The pier, providing foundational support for the road river bridge."
            contains 3 elements
              1 x IFCCOLUMN | type IFCCOLUMNTYPE "road river bridge pierstem" | object type "pierstem" | names: "road river bridge pierstem" | descriptions: "A sturdy pierstem, providing vertical support for the road river bridge." | material: "stone_granite_masonry" | property sets: Qto_ColumnBaseQuantities
              1 x IFCFOOTING | type IFCFOOTINGTYPE "foundation - bridge road" | names: "foundation - bridge road" | descriptions: "A solid foundation, providing support for the bridge rail." | material: "concrete_reinforced_in-situ"
              1 x IFCBEAM | type IFCBEAMTYPE "bridge road - cross girder" | object type "piercap" | names: "bridge road - cross girder" | descriptions: "A robust girder, ensuring stability and support for the bridge road." | material: "wood-generic" | property sets: Qto_BeamBaseQuantities
          IFCBRIDGEPART "road river bridge - pier" | object type "pier" | PARTIAL | LATERAL | PIER | description "The pier, providing foundational support for the road river bridge."
            contains 3 elements
              1 x IFCCOLUMN | type IFCCOLUMNTYPE "road river bridge pierstem" | object type "pierstem" | names: "road river bridge pierstem" | descriptions: "A sturdy pierstem, providing vertical support for the road river bridge." | material: "stone_granite_masonry" | property sets: Qto_ColumnBaseQuantities
              1 x IFCFOOTING | type IFCFOOTINGTYPE "foundation - bridge road" | names: "foundation - bridge road" | descriptions: "A solid foundation, providing support for the bridge rail." | material: "concrete_reinforced_in-situ"
              1 x IFCBEAM | type IFCBEAMTYPE "bridge road - cross girder" | object type "piercap" | names: "bridge road - cross girder" | descriptions: "A robust girder, ensuring stability and support for the bridge road." | material: "wood-generic" | property sets: Qto_BeamBaseQuantities
          IFCBRIDGEPART "road river bridge - pier" | object type "pier" | PARTIAL | LATERAL | PIER | description "The pier, providing foundational support for the road river bridge."
            contains 3 elements
              1 x IFCCOLUMN | type IFCCOLUMNTYPE "road river bridge pierstem" | object type "pierstem" | names: "road river bridge pierstem" | descriptions: "A sturdy pierstem, providing vertical support for the road river bridge." | material: "stone_granite_masonry" | property sets: Qto_ColumnBaseQuantities
              1 x IFCFOOTING | type IFCFOOTINGTYPE "foundation - bridge road" | names: "foundation - bridge road" | descriptions: "A solid foundation, providing support for the bridge rail." | material: "concrete_reinforced_in-situ"
              1 x IFCBEAM | type IFCBEAMTYPE "bridge road - cross girder" | object type "piercap" | names: "bridge road - cross girder" | descriptions: "A robust girder, ensuring stability and support for the bridge road." | material: "wood-generic" | property sets: Qto_BeamBaseQuantities
    IFCSITE "rail river bridge - site" | PARTIAL | elevation above sea level 0. | description "The site of the rail river bridge, facilitating train crossings."
      IFCBRIDGE "rail bridge" | object type "arched" | ARCHED | description "A strong rail bridge, supporting trains as they cross over."
        IFCBRIDGEPART "rail bridge - substructure" | object type "substructure" | COMPLEX | LATERAL | SUBSTRUCTURE | description "The substructure, providing essential support for the rail bridge."
          IFCBRIDGEPART "rail bridge - pier" | object type "pier" | PARTIAL | LATERAL | PIER | description "A sturdy pier, providing foundational support for the rail bridge."
            contains 2 elements
              1 x IFCCOLUMN | type IFCCOLUMNTYPE "rail bridge - pierstem" | object type "pierstem" | names: "rail bridge - pierstem" | descriptions: "A pierstem, providing vertical support for the bridge rail." | material: "stone_granite_masonry" | property sets: Qto_ColumnBaseQuantities
              1 x IFCFOOTING | type IFCFOOTINGTYPE "foundation - bridge rail" | names: "foundation - bridge rail" | descriptions: "A solid foundation, providing support for the bridge rail." | material: "concrete_reinforced_in-situ"
          IFCBRIDGEPART "rail bridge - pier" | object type "pier" | PARTIAL | LATERAL | PIER | description "A sturdy pier, providing foundational support for the rail bridge."
            contains 2 elements
              1 x IFCCOLUMN | type IFCCOLUMNTYPE "rail bridge - pierstem" | object type "pierstem" | names: "rail bridge - pierstem" | descriptions: "A pierstem, providing vertical support for the bridge rail." | material: "stone_granite_masonry" | property sets: Qto_ColumnBaseQuantities
              1 x IFCFOOTING | type IFCFOOTINGTYPE "foundation - bridge rail" | names: "foundation - bridge rail" | descriptions: "A solid foundation, providing support for the bridge rail." | material: "concrete_reinforced_in-situ"
        IFCBRIDGEPART "railbridge - superstructure" | object type "superstructure" | LATERAL | SUPERSTRUCTURE | description "The superstructure, forming the main body of the rail bridge."
          contains 10 elements
            2 x IFCWALL | type IFCWALLTYPE "rail bridge - spandrel wall" | object type "solidwall" | names: "rail bridge - spandrel wall" | descriptions: "A spandrel wall, providing structural support for the rail bridge." | material: "stone_granite_masonry"
            2 x IFCSIGN | type IFCSIGNTYPE "road rail bridge - name sign" | object type "pictoral" | names: "road rail bridge - name sign" | descriptions: "Ye Olde Brygge's Timeless Plaque: A Gleaming Tribute to Bygone Eras" | material: "metal_copper_generic"
            4 x IFCMEMBER | type IFCMEMBERTYPE "rail bridge - arch segment" | object type "arch_segment" | names: "rail bridge - arch segment" | descriptions: "An arch segment, forming part of the rail bridge's structure." | material: "stone_granite_masonry"
            2 x IFCEARTHWORKSFILL | object type "backfill" | BACKFILL | names: "rail bridge - filler" | descriptions: "The filling material between the arches and the bridge deck." | material: "bulk-material_soil_generic"
    IFCSITE "road rail bridge - site" | PARTIAL | elevation above sea level 0. | description "The site of the road rail bridge, supporting both road and rail traffic."
      contains 2 elements
        2 x IFCELEMENTASSEMBLY | type IFCELEMENTASSEMBLYTYPE "highway location marker" | object type "signalassembly" | FACTORY | names: "highway location marker" | descriptions: "A marker indicating specific locations along the highway."
      IFCBRIDGE "rail bridge" | object type "arched" | ARCHED | description "A strong rail bridge, supporting trains as they cross over."
        IFCBRIDGEPART "rail bridge - substructure" | object type "substructure" | COMPLEX | LATERAL | SUBSTRUCTURE | description "The substructure, providing essential support for the rail bridge."
          IFCBRIDGEPART "rail bridge - pier" | object type "pier" | PARTIAL | LATERAL | PIER | description "A sturdy pier, providing foundational support for the rail bridge."
            contains 2 elements
              1 x IFCCOLUMN | type IFCCOLUMNTYPE "rail bridge - pierstem" | object type "pierstem" | names: "rail bridge - pierstem" | descriptions: "A pierstem, providing vertical support for the bridge rail." | material: "stone_granite_masonry" | property sets: Qto_ColumnBaseQuantities
              1 x IFCFOOTING | type IFCFOOTINGTYPE "foundation - bridge rail" | names: "foundation - bridge rail" | descriptions: "A solid foundation, providing support for the bridge rail." | material: "concrete_reinforced_in-situ"
          IFCBRIDGEPART "rail bridge - pier" | object type "pier" | PARTIAL | LATERAL | PIER | description "A sturdy pier, providing foundational support for the rail bridge."
            contains 2 elements
              1 x IFCCOLUMN | type IFCCOLUMNTYPE "rail bridge - pierstem" | object type "pierstem" | names: "rail bridge - pierstem" | descriptions: "A pierstem, providing vertical support for the bridge rail." | material: "stone_granite_masonry" | property sets: Qto_ColumnBaseQuantities
              1 x IFCFOOTING | type IFCFOOTINGTYPE "foundation - bridge rail" | names: "foundation - bridge rail" | descriptions: "A solid foundation, providing support for the bridge rail." | material: "concrete_reinforced_in-situ"
        IFCBRIDGEPART "railbridge - superstructure" | object type "superstructure" | LATERAL | SUPERSTRUCTURE | description "The superstructure, forming the main body of the rail bridge."
          contains 10 elements
            2 x IFCWALL | type IFCWALLTYPE "rail bridge - spandrel wall" | object type "solidwall" | names: "rail bridge - spandrel wall" | descriptions: "A spandrel wall, providing structural support for the rail bridge." | material: "stone_granite_masonry"
            2 x IFCSIGN | type IFCSIGNTYPE "road rail bridge - name sign" | object type "pictoral" | names: "road rail bridge - name sign" | descriptions: "Ye Olde Brygge's Timeless Plaque: A Gleaming Tribute to Bygone Eras" | material: "metal_copper_generic"
            4 x IFCMEMBER | type IFCMEMBERTYPE "rail bridge - arch segment" | object type "arch_segment" | names: "rail bridge - arch segment" | descriptions: "An arch segment, forming part of the rail bridge's structure." | material: "stone_granite_masonry"
            2 x IFCEARTHWORKSFILL | object type "backfill" | BACKFILL | names: "rail bridge - filler" | descriptions: "The filling material between the arches and the bridge deck." | material: "bulk-material_soil_generic"
    IFCSITE "road - site" | PARTIAL | elevation above sea level 0. | description "A designated parking area, providing space for vehicles."

Types
  IFCBUILDINGELEMENTPROXYTYPE "geo-reference" | element type "origin" | USERDEFINED | 1 occurrence | description "The reference point for transforming the local engineering coordinate system into the coordinate reference system of the underlying map."
  IFCSLABTYPE "bridge road - approach slab" | APPROACH_SLAB | 2 occurrences | description "A solid slab, ensuring a smooth transition, the bridge's welcome mat."
  IFCBEAMTYPE "road river bridge - abutment support beam" | element type "beam" | BEAM | 2 occurrences | description "A strong support beam, providing stability to the bridge abutment."
  IFCRAILINGTYPE "bridge road railing" | element type "guardrail" | GUARDRAIL | 2 occurrences | description "A protective railing, ensuring safety along the bridge road."
  IFCSLABTYPE "road river bridge - bridge deck" | element type "floor" | FLOOR | 1 occurrence | description "The bridge deck, providing a stable surface for vehicles to cross the river."
  IFCBEAMTYPE "road river bridge - main girder" | element type "girder_segment" | GIRDER_SEGMENT | 3 occurrences | description "The main girder, providing essential support for the road river bridge."
  IFCCOLUMNTYPE "road river bridge pierstem" | element type "pierstem" | PIERSTEM | 3 occurrences | description "A sturdy pierstem, providing vertical support for the road river bridge."
  IFCFOOTINGTYPE "foundation - bridge road" | PAD_FOOTING | 3 occurrences | description "A solid foundation, providing support for the bridge rail."
  IFCBEAMTYPE "bridge road - cross girder" | element type "piercap" | PIERCAP | 3 occurrences | description "A robust girder, ensuring stability and support for the bridge road."
  IFCCOLUMNTYPE "rail bridge - pierstem" | element type "pierstem" | PIERSTEM | 4 occurrences | description "A pierstem, providing vertical support for the bridge rail."
  IFCFOOTINGTYPE "foundation - bridge rail" | PAD_FOOTING | 4 occurrences | description "A solid foundation, providing support for the bridge rail."
  IFCWALLTYPE "rail bridge - spandrel wall" | element type "solidwall" | SOLIDWALL | 4 occurrences | description "A spandrel wall, providing structural support for the rail bridge."
  IFCSIGNTYPE "road rail bridge - name sign" | element type "pictoral" | PICTORAL | 4 occurrences | description "Ye Olde Brygge's Timeless Plaque: A Gleaming Tribute to Bygone Eras"
  IFCMEMBERTYPE "rail bridge - arch segment" | element type "arch_segment" | ARCH_SEGMENT | 8 occurrences | description "An arch segment, forming part of the rail bridge's structure."
  IFCELEMENTASSEMBLYTYPE "highway location marker" | element type "signalassembly" | SIGNALASSEMBLY | 2 occurrences | description "A marker indicating specific locations along the highway."

Property sets
  Qto_BeamBaseQuantities | quantities | on 3 objects (3 IFCBEAM)
    CrossSectionArea = 0.12000000000000037 [SQUARE_METRE]
    Length = 4000.0000000000005 [MILLI METRE]
    NetVolume = 0.4800000000000016 [CUBIC_METRE]
  Qto_BeamBaseQuantities | quantities | on 1 object (1 IFCBEAM)
    NetVolume = 0.3461128140335334 [CUBIC_METRE]
  Qto_BeamBaseQuantities | quantities | on 1 object (1 IFCBEAM)
    NetVolume = 0.34611281403353333 [CUBIC_METRE]
  Qto_SlabBaseQuantities | quantities | on 1 object (1 IFCSLAB)
    Depth = 200.00000000000003 [MILLI METRE]
    NetArea = 8.767066677832185 [SQUARE_METRE]
    NetVolume = 1.7534133355664374 [CUBIC_METRE]
  Qto_SlabBaseQuantities | quantities | on 1 object (1 IFCSLAB)
    Depth = 200.00000000000003 [MILLI METRE]
    NetArea = 8.767066677832183 [SQUARE_METRE]
    NetVolume = 1.7534133355664372 [CUBIC_METRE]
  Qto_SlabBaseQuantities | quantities | on 1 object (1 IFCSLAB)
    Depth = 55.999999999999986 [MILLI METRE]
    NetArea = 33.373512000000055 [SQUARE_METRE]
    NetVolume = 1.8689166720000028 [CUBIC_METRE]
  Qto_ColumnBaseQuantities | quantities | on 4 objects (4 IFCCOLUMN)
    NetVolume = 24.950281166526725 [CUBIC_METRE]
  Qto_ColumnBaseQuantities | quantities | on 3 objects (3 IFCCOLUMN)
    NetVolume = 4.526915656682752 [CUBIC_METRE]