IFC building model
Schema: "IFC4X3_ADD2"
Description: "ViewDefinition [ReferenceView]"
File name: "Infra-Rail.ifc"
Time stamp: "2024-11-14T11:09:37"
Preprocessor: "IFC-manager for SketchUp (5.3.3)"
Originating system: "SketchUp 2024 (24.0.594)"
Authorization: "None"
Application: "IFC manager for sketchup" version "5.3.3" identifier "su_ifcmanager" by Organization "BIM-Tools"

People and organizations
  Person "Jan B." id "3720f2e9-0107-4ce6-b699-e20d9bd03331" of Organization "buildingSMART International" description "buildingSMART is the worldwide industry body driving the digital transformation of the built environment."
  Owner history of Person "Jan B." id "3720f2e9-0107-4ce6-b699-e20d9bd03331" of Organization "buildingSMART International" description "buildingSMART is the worldwide industry body driving the digital transformation of the built environment." | application "IFC manager for sketchup" version "5.3.3" identifier "su_ifcmanager" by Organization "BIM-Tools" | change ADDED | created 1731578977 (2024-11-14T10:09:37Z) | last modified 1731578977 (2024-11-14T10:09:37Z) by Person "Jan B." id "3720f2e9-0107-4ce6-b699-e20d9bd03331" of Organization "buildingSMART International" description "buildingSMART is the worldwide industry body driving the digital transformation of the built environment." with "IFC manager for sketchup" version "5.3.3" identifier "su_ifcmanager" by Organization "BIM-Tools"

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE

Spatial structure
IFCPROJECT "ifc silly sample scene - project" | description "Demystifying IFC with a playful scene using diverse building elements and compositions."
  IFCSITE "environment - site" | COMPLEX | elevation above sea level 0. | description "A sample scene environment, showcasing the surrounding landscape."
    contains 1 element
      1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "geo-reference" | object type "origin" | names: "geo-reference" | descriptions: "The reference point for transforming the local engineering coordinate system into the coordinate reference system of the underlying map." | material: "virtual_black"
    IFCSITE "road parking - site" | PARTIAL | elevation above sea level 0. | description "A designated parking area, providing space for vehicles."
    IFCSITE "road river bridge - site" | PARTIAL | elevation above sea level 0. | description "The site of the road river bridge, connecting different areas."
    IFCSITE "rail river bridge - site" | PARTIAL | elevation above sea level 0. | description "The site of the rail river bridge, facilitating train crossings."
      IFCRAILWAY "Rail track" | object type "track" | description "Durable rail tracks, guiding trains safely along their path."
        IFCRAILWAYPART "Rail track" | object type "track" | LONGITUDINAL | TRACK | description "Durable rail tracks, guiding trains safely along their path."
          contains 36 elements
            2 x IFCRAIL | type IFCRAILTYPE "rail" | object type "rail" | names: "rail" | descriptions: "Strong rails, guiding trains safely along their path." | material: "metal_hot-rolled-steel"
            1 x IFCCOURSE | type IFCCOURSETYPE "ballastbed" | object type "ballastbed" | names: "ballastbed" | descriptions: "A sturdy ballast bed, providing a stable base for railway tracks." | material: "bulk-material_ballast_generic"
            33 x IFCTRACKELEMENT | type IFCTRACKELEMENTTYPE "sleeper wood" | object type "sleeper" | names: "sleeper wood" | descriptions: "Durable wooden sleepers, supporting the railway tracks." | material: "wood-generic"
    IFCSITE "road rail bridge - site" | PARTIAL | elevation above sea level 0. | description "The site of the road rail bridge, supporting both road and rail traffic."
      contains 2 elements
        2 x IFCELEMENTASSEMBLY | type IFCELEMENTASSEMBLYTYPE "highway location marker" | object type "signalassembly" | FACTORY | names: "highway location marker" | descriptions: "A marker indicating specific locations along the highway."
      IFCRAILWAY "Rail track" | object type "track" | description "Durable rail tracks, guiding trains safely along their path."
        IFCRAILWAYPART "Rail track" | object type "track" | LONGITUDINAL | TRACK | description "Durable rail tracks, guiding trains safely along their path."
          contains 36 elements
            2 x IFCRAIL | type IFCRAILTYPE "rail" | object type "rail" | names: "rail" | descriptions: "Strong rails, guiding trains safely along their path." | material: "metal_hot-rolled-steel"
            1 x IFCCOURSE | type IFCCOURSETYPE "ballastbed" | object type "ballastbed" | names: "ballastbed" | descriptions: "A sturdy ballast bed, providing a stable base for railway tracks." | material: "bulk-material_ballast_generic"
            33 x IFCTRACKELEMENT | type IFCTRACKELEMENTTYPE "sleeper wood" | object type "sleeper" | names: "sleeper wood" | descriptions: "Durable wooden sleepers, supporting the railway tracks." | material: "wood-generic"
    IFCSITE "road - site" | PARTIAL | elevation above sea level 0. | description "A designated parking area, providing space for vehicles."

Types
  IFCBUILDINGELEMENTPROXYTYPE "geo-reference" | element type "origin" | USERDEFINED | 1 occurrence | description "The reference point for transforming the local engineering coordinate system into the coordinate reference system of the underlying map."
  IFCRAILTYPE "rail" | element type "rail" | RAIL | 4 occurrences | description "Strong rails, guiding trains safely along their path."
  IFCCOURSETYPE "ballastbed" | element type "ballastbed" | BALLASTBED | 2 occurrences | description "A sturdy ballast bed, providing a stable base for railway tracks."
  IFCTRACKELEMENTTYPE "sleeper wood" | element type "sleeper" | SLEEPER | 66 occurrences | description "Durable wooden sleepers, supporting the railway tracks."
  IFCELEMENTASSEMBLYTYPE "highway location marker" | element type "signalassembly" | SIGNALASSEMBLY | 2 occurrences | description "A marker indicating specific locations along the highway."